
























ISM ANTENNA



Antenna ISM Connector Mount G015,  
868 MHz, 2 dBi, SMA(m) 90°

AO-A868-G015-RS

SECTRON company oﬀers a wide portfolio of ISM antennas with various versions diﬀering in shape, level of gain and manner of attachment. SECTRON guarantees a compatible connection between   
an antenna and all antenna adaptors produced by SECTRON.

BENEFITS

Low VSWR

Easy installation


AO-A868-G015-RS5

FEATURES

FEATURES

FEATURES

|  |  |
| --- | --- |
| Technology | ISM/LoRa/SIGFOX |
| Frequency bands | 868 MHz |
| Bandwidth | - |
| Gain | 2 dBi |
| VSWR | <2.0:1 |
| Impedance | 50 Ohm |
| Directivity | Omnidirectional |
| Beam angle | H 360° V 30° |
| Polarization | Linear |
| Maximum input power | 10 W |
| Power voltage | - |
| Dimensions | 87.2 x 16.8 x 9.2 mm |
| Weight | 8.34g |
| Operating temperature | -40 to +85 °C |
| Execution | External |
| Method of attachment | Connector Mount |
| Cable type | - |
| The cable length | - |
| Connector type | SMA(m) |



DRAWING

CONTACTS

|  |  |
| --- | --- |
| SECTRON s.r.o. Josefa Šavla 1271/12 | WWW.SECTRON.CZ |
| 709 00 Ostrava 9, Czech Republic | Tel.: +420 556 621 020 |

AO-A868-G015-RS

FEATURES

ALL VARIANTS

|  |  |
| --- | --- |
| VARIANT | PART NUMBER |
|  |  |

CONTACTS

SECTRON s.r.o. Josefa Šavla 1271/12 709 00 Ostrava 9, Czech Republic

[WWW.SECTRON.CZ](http://WWW.SECTRON.CZ/)

Tel.: +420 556 621 021